Readme for camera firmware 

Target platforms:    PD5004, PD5004W
CPU firmware:        v20260312
Pan/Tilt firmware:   v20260306

IMPORTANT NOTICE:
This zip file ships 2x firmware files, one for the main board in the camera and one for the pan/tilt controller board in the camera. 
For these 2x firmware files, two separate steps will need to be taken to completely perform the firmware upgrade:
1) Upgrade the Pan/Tilt firmware using file *-pantilt-firmware-v*.tkhfw
   After upgrading this firmware, the camera will take a reboot time, and then will be ready for the next step.
2) Upgrade CPU firmware using file *-firmware-v*.tkhfw
   After this step, the camera will reboot, after which a 10-15 minutes internal timer runs. During this period, the camera will not accept another CPU firmware upgrade procedure. This is a security feature.
The order in which these steps are performed is important, but both steps must be performed.
If you use the camera's web pages, then the above writing is highly relevant to you.
If you use the SDM2 Device Manager tool, then all you do is select the folder in which the firmwares are located, and SDM2 will take care of the rest.

Changes:
Initial revision

Known issues:
- TODO: ADD: Missing 4th stream dedicated to the distortion-free display of D1/4CIF resolution video
- TODO: ADD: Compass user-defined directional OSD texts
- TODO: ADD: Image stabilization

----------------------------------------------------------------
