A&E SPECIFICATION

BL1103M1-EI
3 MEGAPIXEL INTELLIGENT IP NETWORK BULLET CAMERA WITH IR FOR OUTDOOR
TECHNICAL SPECIFICATIONS		SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

PART 2 - PRODUCTS
2.1	GENERAL
A.	This product shall be manufactured by a firm whose quality system is in compliance with the ISO-9001
B.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
C.	All systems and components shall have been thoroughly tested and proven in actual use.
D.	All systems and components shall be provided with comprehensive repair and spare parts replacement. The manufacturer on warranty and non-warranty items shall guarantee the spare parts and the repair.
E.	All systems and components must be in compliance with FCC, CE, UL and RoHS requirements.
F.	All materials furnished under this item shall be compliant with 802.3at Ethernet standards 
2.2	HD 3 MEGAPIXEL NETWORK Bullet CAMERA
A.	The network camera shall offer three video streams with up to 3MP resolution (2048 × 1536) in progressive scan CMOS format, with H.264 video compression.
B.	The network camera shall provide true & day night (ICR) low-light capabilities with sensitivity down to Color: 0.05 lux @ (F1.2, AGC ON); B/W: 0.005 lux @ (F1.2, AGC ON); 0 lux with IR.
C.	The network camera shall support Back-Light Compensation (BLC) with selectable zones.
D.	The camera shall offer video compression of H.264 and MJPEG. Three H.264 streams shall be supported with independent resolution, bit rate and frame rates for the main, sub and third streams.
E.	The network camera shall support enhanced H.264i compression to reduce bandwidth requirements.
F.	The network camera shall include embedded Linux OS and support IE and client software for network preview, and be capable of performing firmware upgrades through a network using a software-based device utility or through the web interface.
G.	The network camera shall be equipped with built-in password protection which is not dependent on a server.
H.	The network camera shall not require a password during installation phase. Password protection will be activated after an administrator user account has been created.
I.	The network camera shall support standard IT protocols including: TCP/IP,ICMP,HTTP,HTTPS,FTP,DHCP,DNS,DDNS,RTP,RTSP,RTCP,PPPoE,NTP,UPnP, SMTP,SNMP,IGMP,802.1X,QoS,IPv6,Bonjour.
J.	The network camera shall support industry standard Power over Ethernet (PoE) IEEE 802.3af Class 3 for powering the camera over the network in addition to 12 Vdc local power.
K.	The camera shall provide the ability to take snapshot and record video clips from the web interface and store on the local computer.
L.	The camera shall support video motion detection with user defined areas and configurable sensitivity levels. In addition, the motion detection shall be supported by an arming schedule with the audible warning, surveillance center notification, email, ftp upload, and alarm output triggered as supported events.
M.	The camera’s web interface shall permit settings to be exported to and imported from a configuration file via the web interface and API.
N.	The camera shall conform to ONVIF, PSIA, CGI and ISAPI standards for integration with 3rd party video management systems (VMS). The camera may also support custom firmware for specific integration with a 3rd party VMS.
2.3	    PoWER
A.	Power Supply		12 Vdc ± 10%, PoE (802.3af Class 3)
B.	Power Consumption		Max. 12 W
2.4	Camera
A.	Image Sensor 		1/2.8” Progressive Scan CMOS
B.	Min. Illumination 		Color: 0.05 Lux @ (F1.2, AGC ON); 
				B/W: 0.005 Lux @ (F1.2, AGC ON), 0 lux with IR
C.	Shutter Time 		1s to 1/100,000s
D.	Iris Mode		DC drive
E.	Lens		2.8-12mm, angle of view: 94.5° - 30.5°
F.	Lens Mount		AF automatic focusing and motorized zoom lens
G.	Max. Image Resolution 		2048 × 1536
H.	Resolutions supported	Main Stream: 
		50Hz: 45fps (2048 × 1536), 50fps@ (1920 × 1080, 1280 x 720)
		60Hz: 45fps (2048 × 1536), 60fps@ (1920 × 1080, 1280 x 720)
	  	Sub Stream: (4CIF, CIF, VGA)@25/30fps
Third Stream: (1280 × 720, 4CIF, CIF, VGA)@10fps
I.	 Day & Night	Day, Night, Auto, Schedule, Triggered by alarm input are 
		selectable in Day/night Switch; two group of parameters can 
		be set respectively for day and night
J	 IR	Enable or Close
K.	 Sensitivity	If you choose auto day/night switch, you can choose the 
		sensitivity of the switch as high, normal and low
L. 	 WDR	Wide dynamic range can be used when there is a high contrast 
		of the bright area and the dark area of the scene, 120dB
M.	 BLC Area	BLC area is the area sense the light intensity; Close, Up, 
		Down, Left, Right and Center are selectable
N.  Back Light Compensation	On/ Off, Zone configurable
O.	Digital Noise Reduction		Off, Normal Mode and Expert Mode are selectable
P.	Noise Reduction Level		For adjusting the noise reduction level and only valid when the 
				DNR function is enabled
Q.	Scene Mode:		Choose the scene as indoor or outdoor.
R.	Image Settings	Saturation, Brightness, Contrast, Sharpness
S. 	Image rotation		Mirror (Left/Right, Up/Down, Center, Close)
T. 	White Balance		MWB, AWB1, AWB2, Locked WB, Fluorescent Lamp, 
			Incandescent Lamp, Warm Light Lamp, Natural Light
U.	Target Cropping		Providing more details of the target area in the third stream
V.	Distortion Correction		Automatically correct the aberrations in image

2.5	VIDEO & Audio SPECIFICATIONS
A.	Compression		      	Main stream: H.264
                            	Sub stream: H.264, MJPEG
							 	Third stream: H.264, MJPEG
B.  Three Streams 		Yes; Main stream up to 2048×1536; sub-stream up to 4CIF; 
				third stream up to 1280×720
C.  Video Bit Rate		32 Kbps ~ 16 Mbps
D.  Audio Compression		G.711/G.722.1/G.726/MP2L2
E.  Audio Bit Rate           		64 Kbps (G.711) /16 Kbps (G.722.1) / 16Kbps (G.726) / 
				32-128 Kbps (MP2L2)
F.  Rate Control		      	Constant, Variable
G. 	H.264 profiles		      	Base Line Profile / Main Profile / High Profile
								H.264i intelligent compression
H.	Max. Frame Rate(main)   	45fps@2048×1536
I.	Sub-stream           	  	4CIF, CIF, VGA
J.	Third-stream			  	1280 × 720, 4CIF, CIF, VGA
K.	Users
	1. Unicast		          	Up to 20 simultaneous users
	2. Multicast			      	Unlimited H.264
L.	Security Access		      	Password protected
M.	Software Interface	      	Web browser view and remote client.
2.6	Network
A.	Alarm Trigger 	     		Motion detection, tampering alarm, network disconnect, IP 
				address conflict, storage exception
B.	Protocols 	     		TCP/IP, ICMP, HTTP,HTTPS, FTP, DHCP,DNS, DDNS, RTP, 
					RTSP, RTCP, PPPoE, NTP, UPnP, SMTP, SNMP, IGMP, 
					802.1X, QoS, IPv6, Bonjour
C.  Security                  	User authentication, watermark, IP address filtering, 
					Anonymous access
D.  System Compatibility	   	ONVIF, PSIA, CGI, ISAPI
E.	Communication Interface 		1 RJ45 10 M/100 M/1000 M Ethernet port
F.  On-board storage          	Built-in Micro SD/SDHC/SDXC card slot, up to 128 GB
2.7	INTELLIGENT FEATURES
A.	Motion Detection 	     		Normal mode and expert mode are available. In expert mode, 
				sensitivity and proportion of motion detection can be set for 8 
				regions and day or night
B.	Face Detection 	     		Human face that appears in the image can be recognized and 
					trigger e-mail, center or FTP linkage, and sensitivity of which 
					can be adjusted
C.  Audio Exception Detection  	As the sound of environment is abnormal, the device can 
recognize it and trigger alarm output
D.  Intrusion Detection  		4 regions of rectangular area can be set with different 
threshold, sensitivity and percentage
E.	Line Crossing Detection		4 lines can be set with different sensitivity to detect line 
				crossing behavior
F.	Region Entrance Detection		Enter a pre-defined virtual region from the outside place
G. 	Region Exiting Detection		Exit from a pre-defined virtual region
H. 	Unattended Baggage		Objects left over in the pre-defined region such as the
					purse, dangerous materials
I.		Object Removal		Objects removed from the pre-defined region, such as the 
					exhibits on display.
J.  Defocus Detection         	If focus of camera is changed, device can trigger alarm output
K.  Scene Change Detection		Arming schedule can be set for scene change detection; alarm 
				output can be linked
L.  ROI		Region of interest can be set as fixed area
M.	Defog		Defog can be turned on to get clear image in fog or haze
N.	VCA		VCA information can be written in streams, and back-end 
				devices can search for video clips contain specified type of 
				events
O.	Object Counting		Entrance and Exit object number is accounted and showed on 
					screen in real time (day/month/year based data chart can be 
					exported)
2.8	Web Browser Requirements
A.	Operating System		PC (Intel® Core® 2 Duo microprocessor, 2.6 GHz) with 
			Microsoft® Windows® XP, Windows Vista®, or Windows® 7 
B.	Web User Interface		   	DirectX for Windows XP, Windows Vista, Windows 7
C.	RAM 		                	2 GB
D.	Ethernet Card 		       	100 Mbps
E.	Web Brower		       	Internet Explorer® 7.0 or later; Firefox, Chrome
F. 	Screen Resolution 		   	1024 x 768 pixels or higher, 16- or 32-bit pixel color resolution
2.9	PHYSICAL
A. 	Operating Conditions		-30 °C ~ 60 °C (-22 °F ~ 140 °F) 
B.	Humidity		95% or less (non-condensing)
C.	IR Range			Up to 50 meters
C. 	Dimension 		100 × 103.9 × 311.8 mm (3.94” × 4.09” × 12.28”)	
D.	Weight 		2000 g (4.41 lbs)
E. 	Construction
a.	Body Material		   	Aluminum alloy
b.	Body Color		       	RAL 9003
c.	Screws		           	Stainless Steel, Security Torx
2.10	certifications and ratings
A.	Regulatory
a.	IEC/EN 61000
b.	IEC/EN 55022 
c.	IEC/EN 55024
d.	IEC /EN60950-1
e.	FCC Part 15, Class b
f.	UL/cUL 60950-1
g.	RoHS
B. 	Ratings
a.	Ingress Protection 	IP67

2.11	Models
BL1103M1-EI