TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

PART 2 - PRODUCTS
2.01	 GENERAL
A.	This product shall be manufactured by a firm whose quality system is in compliance with the ISO-9001 (2008)
B.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
C.	All systems and components shall have been thoroughly tested and proven in actual use.
D.	All equipment shall be new, corrosion resistant and in strict accordance with the details shown on the plans and in the specifications.
E.	All materials furnished under this item shall be compliant with 802.3 Ethernet standards 
F.	All encoders and decoders shall be of the same manufacturer.
G.	All systems and components shall be provided with comprehensive repair and spare parts replacement. The manufacturer on warranty and non-warranty items shall guarantee the spare parts and the repair.

2.02 	Four Channel Encoder
A.	The EVE FOUR is a four channel encoder  providing four (4) video channels, terminal server operation for one (1) RS data channel, four (4) audio in channels, one audio out channels and eight (8) I/O contacts over 10/100BASE-TX or 100BASE-FX Ethernet network
B.	The Four Channel Encoder shall be a mountable on a DIN RAIL.  
C.	The Four Channel Encoder shall have an operational temperature of 0 to +50C and humidity 95% (non condensing) without using fans or any other moving parts . 
D.	The Four Channel Encoder shall have an option to be powered by IEEE 802.3af Power over Ethernet.
E.	The Four Channel Encoder is a dual-stream encoder capable of simultaneously streaming dual H.264 and/or MJPEG streams. 
F.	The Four Channel Encoder shall provide two independent digital video streams, per encoder type, with different resolutions, frame rates, and bit rates. 
G.	The Four Channel Encoder shall support H.264 and MJPEG for compression methods with a maximum resolution of 960x576.  
H.	The Four Channel Encoder shall compress the incoming video using H.264 HP and support MJPEG. 
I.	The Four Channel Encoder shall utilize a comb filter in order to produce high quality video images with fine details. Use of notch filter shall not be acceptable. 
J.	The Four Channel Encoder shall provide sophisticated deinterlacing modes which utilize both linear and non-linear interpolation. In addition it shall be able to filter noise by a 3D noise filter
K.	The Four Channel Encoder shall support streaming over RTP/UDP/IP, multicast and unicast connections for audio and video and RTSP/RTP/TCP/IP for video. In addition to hardware decoding, the encoder shall be interoperable with standard software decoders such as Video LAN’s VLC media player.
L.	The Four Channel Encoder shall support Session Announcement Protocol (SAP) for broadcasting multicast session information. An application can use this information to receive an H.264 video stream or audio stream transmitted by the encoder to the advertised multicast address.
M.	The Four Channel Encoder shall provide flood protection mechanism using real time control protocol (RTCP).
N.	The Four Channel Encoder shall provide a full featured web interface for both live viewing and configuration of the video inputs. The Live View page shall provide options for the encoder to be viewed and provide full Pan, Tilt, Zoom, Focus, Iris, and Preset (set and go) controls. 
O.	The user shall be able to remotely reboot the unit, reboot the unit and return the setting to factory defaults leaving the network setting unchanged, or reboot the unit and restore all setting to factory defaults.  To reboot there is a reboot switch accessible thru a pinhole 
P.	The Four Channel Encoder shall provide status and information on the web interface. Status shall include but not be limited to video real-time streaming state. Measurements shall include the noise, contrast, exposure , and focus of the incoming image.
Q.	The Four Channel Encoder shall support a minimum of 3 levels of password protected access: administrator, operator and viewer.
R.	The Four Channel Encoder is based on open streaming architecture (OSA) standards (API) and shall operate in a TKH Security environment as well as in third-party software recording solutions. 
S.	The Four Channel Encoder shall be certified for ONVIF profile S.
T.	The Four Channel Encoder shall provide for configuration of the contrast, brightness, color saturation, hue, and sharpness from the web interface.
U.	The Four Channel Encoder shall provide built in analytics that checks the health of each connected  camera. This image quality monitor analyzes contrast, exposure, sharpness and noise, and immediately alerts an operator for any malfunctioning.
V.	The Four Channel Encoder shall provide tampering detection which can monitor the position of all four cameras or obstructions in the field-of-view of the cameras. The tamper detection alerts an operator of the tamper event.
W.	The Four Channel Encoder shall support an FTP Push function.  The FTP Push function shall enable the encoder to send a jpeg image to a specified client location at user specified intervals, or on user configurable encoder events. 
X.	The Four Channel Encoder shall provide event management for sending events to a digital I/O or an FTP push. Events shall include “No video”, video motion detect, I/O, image quality, tampering events.
Y.	The web interface shall provide the ability to load firmware remotely to the device.  
Z.	Also it shall provide the ability to provide PTZ control to cameras.  The PTZ interface shall accept various, standard camera control protocols, such as Pelco D and Bosch/Phillips.  Additional control protocols shall be capable of being uploaded via the web interface of the encoder.  The web interface shall provide for PTZ control of the camera and preset creation and selection.  Further control of focus and iris control shall be supported from the interface, but will be dependent on the camera and control protocol connected to the encoder.
AA.	The Four Channel Encoder shall support NTP protocol over IP for time synchronization
BB.	The Four Channel Encoder shall meet or exceed the following design and performance specifications.

2.03	ELECTRICAL SPECIFICATIONS
A.	Network interface 				10/100/1000Base-TX RJ-45		
B.	Cabling					Cat-5 Cable or better for 1000Base-TX
C.	Video Input					BNC, 75 ohm, gold-plated center pin
D.	Video termination				75 ohm
E.	Power consumption				7W max
F.	Input Power				11 -19 VDC (12VDC nominal)
G.	Alarm I/O 					Spring loaded termination block
H.	LED Status indicators 			Power, Ethernet /activity

2.04  	VIDEO SPECIFICATIONS
A.	Video Channels			4 Channels 
B.	Video Input format			Auto detect/NTSC/PAL;  Interlaced or progressive
C.	Input Level			1 Vp-p (+/- 3 dB)
D.	Number of video streams 			2x H.264/MJPEG
E.	Digital Signal Processor		Multi core SoC
F.	Streaming Profiles			Encoding is managed by streaming profiles.
G.	Frame rate			1 - 30 frames per second (fps)
H.	Image Processing	Motion Adaptive Deinterlacing (MAD); 3D noise 
		reduction; Fog correction.
I.	Compression algorithm	H.264 High Profile (ISO/IEC MPEG-4 AVC) or MJPEG
J.	Network protocol	H.264, RTP, UDP, IP, DHCP, SSM,  IGMP v2, RTSP, (S)NTP, SDP, MX/IP, HTTP, HTTPS, SAP, UPnP, FTP, Telnet, ONVIF
K.	Resolution
a.	960H
i.	NTSC			960x480
ii.	PAL				960x576
b.	D1
i.	NTSC			720x480
ii.	PAL				720x576
c.	2/3 D1
i.	NTSC			480x480
ii.	PAL 			480x576
d.	½ D1
i.	NTSC			352x480
ii.	PAL				352x576
e.	2CIF
i.	NTSC			720x240
ii.	PAL				720x288
f.	VGA
i.	NTSC/PAL			640x480
g.	CIF
i.	NTSC			352x240
ii.	PAL				350x288

L.	Video motion detection (VMD)			User-defined region of interest and sensitivity 
M.	VMD Alarm response			Via associated software(via API)  or digital I/O
N.	Camera Health 			Focus, Contrast, SNR, Exposure
O.	Tamper Monitoring			Image Positioning
P.	Camera Health and tampering alarms 	Via associated software(via API)  or digital I/O
Q.	Encoding latency			<130 ms typical;
R.	GOP structure			I, P frames with adjustable I frame interval
S.	Number of output streams		20 (RTSP) Max.
T.	Total output data rate 			Up to 50 Mb/s
U.	Encoder bit rate control		Maximum bit rate and long term target bit rate control
V.	Selectable Video profiles			Custom profiles based on Predefined profiles
W.	Video settings			Auto; Contrast, brightness, color saturation, hue, 
				sharpness
X.	Type of streaming			RTP/UDP/IP, (multicast and/or unicast); RTSP/RTP/TCP/IP;
			HTTP/RTSP/RTP/TCP/IP
Y.	On-screen display (OSD)		2x text lines (configurable: position, color, transparency, border/outline color, font size)
Z.	User levels		Support up to 3 levels – viewer, operator and administrator with rights ranging from view webpage video only to full administration.

2.05	AUDIO
A.	Two-way audio				4 Audio inputs, 1 audio output
B.	Sampling Resolution			ITU G.711
C.	Max. Bandwidth				40Hz to 8kHz
D.	Input Level					Channels 1 and 3 selectable line or mic level (incl bias)
Channels 2 and 4 line level
E.	Output Level				Adjustable, 3 VRMS max.
F.	Input Impedance				>10 kOhm unbalanced
G.	Output Impedance				<100 Ohm unbalanced	

2.06	Digital I/O 
A.	Alarm input/output 			8 inputs/outputs, normally open (fail-safe)
B.	Operational modes				Input, Output, Output (inverted), forced closed
C.	Input 					Open collector:  24 Vdc , 1 Adc maximum load 
D.	Output 					Internal pull-up: 3.3 Vdc, 2.2 kΩ; threshold 1.2V
E.	Remote Control				HTTP API (OSA), ONVIF profile S

2.07 	DATA
A.	Data Ports 					1 serial, half duplex port
a.	Port 1					EIA RS-422 send only (2 wire) or EIA RS-485 (2 wire). 
B.	Operation					UART operation. 
C.	Data Rate 					300b/s to 230.4 kbps.
D.	Transport					TCP /IP  terminal server 
E.	PTZ Control Interfaces			Serial Tunneling, Web Page, HTTP (API),
F.	PTZ Control	Protocol -Standard		Pelco-D, Bosch 
G.	Additional Control Protocols		Vicon, Pelco-P, AD (422), Panasonic (Conventional, New); 						Others per project requirement; remotely uploaded as 							required. 

2.08	MECHANICAL SPECIFICATIONS
A.	Dimensions					120 x 40 x 94 mm 
B.	Weight					360 g
C.	Housing					Aluminum die-cast DIN rail
D.	Color					Sky blue

2.09	NETWORK SPECIFICATIONS
A.	RJ45					10/100/1000BASE-TX, CAT-5
B.	Management				OSA HTTP API, MX (limited), HTML (password 							protected); 

2.10	ENVIRONMENTAL SPECIFICATIONS
A.	Operating temperature			0 to +50 °C
B.	Humidity					 to 95% RH, non-condensing
C.	MTBF					>200,000 hrs

2.11	CERTIFICATIONS AND RATINGS
A.	IEC/EN 60950-1
B.	IEC/EN 61000-6-2
C.	IEC/EN 61000-6-3
D.	EN 55022
E.	CE
F.	FCC part 15
G.	RoHS

2.12	MANUFACTURER’S WARRANTY
A.	Repair or replacement of defective parts for a period of 3 years from date of shipment.

2.12	MODELS
A.	Four Channel Encoder, DIN rail mount		EVE FOUR  v1
B.	Four Channel Encoder w/PoE 			EVE FOUR-PoE v1