TECHNICAL SPECIFICATIONS	SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

PART 2 - PRODUCTS
2.01	 GENERAL
A.	This product shall be manufactured by a firm whose quality system is in compliance with the ISO-9001
B.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
C.	All systems and components shall have been thoroughly tested and proven in actual use.
D.	All materials furnished under this item shall be compliant with 802.3 Ethernet
E.	All systems and components shall be provided with comprehensive repair and spare parts replacement. The manufacturer on warranty and non-warranty items shall guarantee the spare parts and the repair.

2.02 	INDOOR/OUTDOOR CCTV CAMERA DOME SYSTEM
A.	The Siqura HSD622 is an indoor/outdoor IP pan/tilt/zoom (PTZ) camera capable of streaming dual streaming H.264 while simultaneously streaming dual MPEG-4/MPEG-2 /MJPEG streams. 
B.	The indoor/outdoor CCTV camera dome system shall provide four independent digital video streams, with different resolutions, frame rates, and bit rates. The CCTV Dome System shall support H.264, MPEG-2, MPEG-4 and MJPEG for compression methods.  For highest quality H.264 performance, the CCTV Camera Dome System shall use a separate processor from the MPEG2/4/MJPEG DSP, for hardware H.264 encoding of the video stream.
C.	Each H.264 and MPEG-2/4/MJPEG stream of the indoor/outdoor CCTV camera dome system shall be capable of being streamed to three different destinations simultaneously for distribution to the video network.  The CCTV Dome System shall simultaneously handle H.264 encoding and dual MPEG-2/4/MJPEG encoding at full frame rate, and a separate Live View (MJPEG) encoder at 5 frames per second.   Each stream can be streamed to different unicast and/or multicast destinations.  The MJPEG Live View shall be present within the web interface and viewed by HTTP.
D.	The indoor/outdoor CCTV camera dome system shall support streaming over RTP/UDP/IP for audio and video, multicast and unicast connections and RTSP/RTP/TCP/IP for video. In addition to hardware decoding, the camera systems shall be interoperable with standard software decoders such as Quick Time and Video LAN’s VLC media player.
E.	The indoor/outdoor CCTV camera dome system shall support Session Announcement Protocol (SAP) for broadcasting multicast session information. An application can use this information to receive an H.264/MPEG-4/-2 video stream or audio stream transmitted by the camera system to the advertised multicast address.
F.	The indoor/outdoor CCTV camera dome system shall provide a Stream Manager to set a maximum network load per stream which limits the output rate to each of the streams transmitters. In addition, the camera system shall provide a minimum of 3 RTP control modes to manage the network load if the receiver fails including no control, a Flood Guard flood protection mechanism and real time control protocol (RTCP).
G.	 The indoor/outdoor CCTV camera dome system shall provide an option to insert metadata in the video stream. This metadata at a minimum shall include video loss, black/white video, video motion detection alarms, tampering alarms, and image quality monitor alarms. In addition, temperature alerts, audio detection alerts and contact closure status shall be provided in metadata format.
H.	The indoor/outdoor CCTV camera dome system shall provide a full featured web interface for both live viewing and configuration of the camera. The Live View page shall provide options for the encoder to be viewed and provide full Pan, Tilt, Zoom, Focus, Iris, and Preset (set and go) as well as On-Screen Menu navigation controls. Volume control for audio shall also be supported.
I.	The user shall be able to remotely reboot the unit, reboot the unit and return the setting to factory defaults leaving the network setting unchanged, or reboot the unit and restore all setting to factory defaults.  
J.	The indoor/outdoor CCTV camera dome system shall provide status and measurement information via the web interface. Status shall include but not be limited to video and audio real-time streaming state. Measurements shall include codec board current and peak temperatures, network tx/rx bit rates, CPU and DSP loading, real-time video bit, frame rates and latency, audio sample rate FTP push status and PTZ coordinates.
K.	The indoor/outdoor CCTV camera dome system shall be able to transmit up to three independent copies of audio signal pairs (one pair in one stream), up to three copies of each of two independent data signals, and up to three copies of each of eight independent contact closure signals, each stream having an independently selectable IP destination
L.	The indoor/outdoor camera system shall support a minimum of 4 levels of password protected access with 3 distinct levels of web page access including administrator, operator and viewer. In addition, the operating system (Linux) shall have configurable root pass code protection with no back door access.
M.	The indoor/outdoor CCTV camera dome system is based on open streaming architecture (OSA) standards (API) and shall operate in a Siqura environment as well as in third-party software recording solutions. In addition, the camera system shall support ONVIF v1.02 or later for open systems compatibility native or as an upgrade.
N.	The indoor/outdoor CCTV camera dome system shall include a removable 100Base-TX network interface for live streaming to a standard Web browser and a analog output for live monitoring.
O.	The indoor/outdoor CCTV camera dome system shall provide a small form-factor pluggable (SFP) interface which can be installed in place of the removable RJ45 interface. This SFP interface shall provide for direct fiber to the dome and support a wide range of SFP fiber modules including Single Mode, Multi-mode and CWDM.
P.	The indoor/outdoor CCTV camera dome system shall be a discreet camera dome system consisting of a integral dome drive with a variable speed/high speed pan/tilt drive unit with continuous 360 rotation (slip ring), 1/4-inch high resolution color/black-white CCD camera, motorized zoom lens with 26x optical and 12x digital zoom, Auto iris and auto focus with manual override control. The indoor/outdoor CCTV camera domes system shall be in an environmental IP66 enclosure, with sunshield as standard offering. The unitized camera body shall connect to a pendant style adapter with quick-install ¼ rotation gasketed interface with locking screw. The pendant adapter shall mount to all mounting brackets with a quick install ¼ rotation interface with locking hardware. 
Q.	The Indoor/Outdoor CCTV camera dome system shall be compatible with a wide range of mounting accessories from the same manufacturer including but not limited to wall, pole, corner, ceiling and an adapter for other manufacturers 1 ½”NPT mounts.
R.	The indoor/outdoor CCTV camera dome system shall provide user commands for controlling key image functions directly from a CCTV keyboard or GUI including Day/Night (Auto, On, Off), Back Light Compensation (On/Off ) and Wide Dynamic Range (On/Off) without entering On-screen Menus or web browser interfaces.
S.	The indoor/outdoor CCTV camera dome system shall provide Pan, Tilt Zoom coordinate positions and permit querying and positioning the unit with such coordinate date via the cameras API. 
T.	The indoor/outdoor CCTV camera dome system shall provide built in analytics that checks the health of the camera. This image quality monitor analyzes contrast, exposure, sharpness and noise, and immediately alerts an operator for any malfunctioning.
U.	The indoor/outdoor CCTV camera dome shall provide tampering detection which can monitor the position of the camera or obstructions in the field-of-view of the camera for up to 16 preset reference images.  After a configurable time period, the tamper detection alerts an operator of the tamper event.
V.	The indoor/outdoor CCTV camera dome system shall support both an FTP Push function, and an FTP pull function.  The FTP Push function shall enable the camera system to send a jpeg image to a specified client location at user specified intervals, or on user configurable encoder events.  The FTP pull function shall enable the camera system to send a jpeg image on request of a remote server.
W.	The indoor/outdoor CCTV camera dome system shall provide event management for sending events to a contact closure stream or an FTP push. Supported event triggers shall include event on, off or changed. Events shall include video, video motion, audio, contact closure, image quality, tampering events.
X.	The indoor/outdoor IP PTZ dome camera system shall meet or exceed the following design and performance specifications.

2.03	ELECTRICAL SPECIFICATIONS
A.	Network interface 				Interchangeable 100Base-TX RJ-45 and 									SFP connector modules
B.	Cabling					Cat-5 Cable or better for 100Base-TX
C.	Analog  output				BNC
D.	Power consumption (/with heater)		27W/ 73W with heater max.
E.	Input Power				19.2 – 28.4 VAC (24 VAC nominal +/- 20%)
							22 -27 VDC (24VDC nominal)
F.	Audio In/Out				3.5mm jacks
G.	Alarm Inputs- 8				Color coded wire harness
H.	Alarm Outputs -1 				Color coded wire harness

2.04  	VIDEO SPECIFICATIONS
A.	Number of video streams 			2x H.264, 2x MPEG-4/MPEG-2 and/or MJPEG
a.	Hardware Based			Two H.264 streams shall be from dedicated 					hardware co-processors.
b.	DSP encoders			A flexible TI DaVinci DSP shall be available to 					provided two selectable software based MPEG-4 or 				MPEG-2 or MJPEG streams.
B.	Encoder Priorities			Encoding priority shall be configurable.
C.	Frame rate			1 - 30 frames per second (fps)
D.	Image processing			Interlaced/Deinterlaced; Deinterlacing shall be 					configurable for edge adaptive and motion adaptive 				modes.
E.	Compression algorithm	H.264 BP (ISO/IEC  14496-10); MPEG-4 SP Layer 5 	(ISO/IEC  14496-2); MPEG-2 (ISO/IEC 13818-	2),MJPEG
F.	Network protocol	H.264 BP, MPEG-4 ES, MPEG-2 (ES or TS),  RTP, UDP, IP, DHCP, SSM,  IGMP v2, RTSP, (S)NTP, SDP, MX/IP, HTTP, SNMP v2, DiffServ, SAP, UPnP, FTP, Telnet
G.	Resolution
a.	D1
i.	NTSC			720x480
ii.	PAL				720x576
b.	2/3 D1
i.	NTSC			480x480
ii.	PAL 			480x576
c.	½ D1
i.	NTSC			352x480
ii.	PAL				352x576
d.	2CIF
i.	NTSC			720x240
ii.	PAL				720x288
e.	VGA
i.	NTSC/PAL			640x480
f.	CIF
i.	NTSC			352x240
ii.	PAL				350x288
g.	QVGA
i.	NTAC/PAL			320x240
h.	QCIF
i.	NTSC			176x120
ii.	PAL				176x144
H.	Video motion detection (VMD)			User-defined free-drawn masking, sensitivity and 				response level; 
I.	VMD Alarm response			Via associated software(via API)  or contact closure
J.	Camera Health 			Focus, Contrast, SNR, Exposure
K.	Tamper Monitoring			Image Positioning (up to 16 presets)
L.	Camera Health and tampering alarms 	Via associated software(via API)  or contact closure
M.	Encoding latency			<130 ms typical; <90 ms (low latency mode)
N.	GOP structure			I, P frames with adjustable I frame interval
O.	Number of output streams 			20 (RTSP) max.
P.	Total output data rate 			Up to 20 MB/s
Q.	Encoder bit rate control		Constant bit rate (CBR), variable bit rate (VBR) or Constant Quality (H.264 only) 
R.	Selectable Video profiles			Custom settings or Predefined profiles optimized, at a 				minimum, for High Quality Camera or PTZ, Storage 				and Low bandwidth.
S.	Stream Priorities			Encoder streams shall be prioritized for optimal 					performance.
T.	Video settings			Contrast, brightness, color saturation, hue, sharpness
U.	Type of streaming		RTP/UDP/IP, (multicast and/or unicast); RTSP/RTP/TCP/IP
V.	On-screen display (OSD)		3x text lines (configurable: position, color, transparency, border/outline color, font size);1x image in BMP, Animated GIF, or JPEG format (configurable: position, scaling)
W.	User levels		Support up to 4 levels – viewer, operator and administrator with rights ranging from view webpage video only to full administration, and “root” for the Linux prompt.

2.05 	CAMERA SPECIFICATIONS
A.	Image sensor				¼” EXview HAD CCD
B.	Scanning system				2:1 Interlaced output
C.	Minimum illumination			0.09 lux (color), 0.01 (B/W), F1.6, ¼ sec shutter, 50IRE
D.	Electronic shutter				½ - 1/10 k s
E.	Horizontal resolution			530 TVL
F.	Optical zoom				26x
G.	Digital zoom				12x
H.	Analog					NTSC or PAL
I.	Video output				1.0 Vpp/75Ω impedance
J.	Effective pixels				768x494 NTSC, 752x582 PAL
1.	NTSC					380k
2.	PAL						440k
K.	Signal noise ratio (SNR)			>50 dB (AGC off)
L.	Focal length				3.5 - 91 mm
M.	Horizontal Field of View			54.2˚ wide to 2.2˚ tele

2.06  	CAMERA OPERATION			
A.	Iris control					Auto/manual
B.	Focus mode					Auto/manual
C.	Zoom					Auto/manual
D.	AGC					Auto/manual
E.	White balance				Auto/manual
F.	Backlight Compensation			Auto/manual
G.	Day/night (IR-cut filter)			Auto/On/off
H.	Digital slow shutter				On/off
I.	Wide dynamic range (WDR)			On/off 
J.	Privacy Masks				24; Zoom factor enabled/disabled

2.07	DOME DRIVE SPECIFICATIONS
A.	Pan travel					360° continuous
B.	Tilt travel					-10° - 190° with configurable limits
C.	Preset speed				400°/s
D.	Manual speed				90°/s
E.	Presets					256 preset commands (228 positions)
F.	Motor Drive				0.9 degree stepper motor with cogged belt drive 
G.	Preset accuracy				+/- .100 deg
H.	Menu system				English,  French, German, Italian, Japanese, Polish, 							Portuguese, Russian, Spanish
I.	Freeze Frame				Freeze current image during preset movement
J.	Cruise					8, with 200 seconds per cruise
K.	Sequence					8
L.	Auto pan					4
M.	Proportional pan and tilt			On/off
N.	Resume after power loss			Yes
O.	Camera ID					Yes (on/off)
P.	Camera Title				Yes
Q.	Preset Title					Yes
R.	Zone title					16
S.	Home function				Preset, sequence, auto pan, cruise
T.	Auto flip					Digital/mechanical/off
U.	PTZ control protocols			OSA API, Bi-directional Pelco-D or NTCIP
V.	OSD Positional				Compass direction, Azimuth, Elevation
W.	PTZ coordinate data				OSA API or Pelco-D
X.	Auto-calibration				Auto/Off/Remote triggered/scheduled

2.08	AUDIO
A.	Two-way audio				Full duplex mono
B.	Sampling Resolution			8bit linear PCM or ITU G.711
C.	Max. Bandwidth				20hz to 20kHz
D.	Input Level					Adjustable, mic or line 
E.	Output Level				Adjustable, 3Vpk-pk
F.	Input Impedance				>20kOhm or 600 Ohm
G.	Output Impedance				<100 Ohm	
H.	Transport					RTP/UDP/IP multicast and unicast
I.	Transmission				Up to 3 independent copies of audio signal pairs with 							each stream having an independently  selectable IP 							destination    

2.09	CONTACT CLOSURES
A.	Alarm input 				8 contact closure inputs, normally open (fail-safe)
B.	Operational modes				Normal, inverted, forced active or forced inactive
C.	Sampling rates				contact closure shall be sampled 100 times per second 							and provide latency of less than 20 msec. 
D.	Transport					 TCP and UDP (unicast or multicast),
E.	Transmission				Independently selectable IP destination and port 							number.
F.	Alarm output				1  contact closure output
G.	 Remote Control				HTTP API (OSA)

2.10	MECHANICAL SPECIFICATIONS
A.	Dimensions					Ø7.5 x 11.9 in (Ø190 x 302.5 mm)
B.	Weight					5.7 lbs. (2.6 kg)
C.	Color					RAL-9003 (Signal White)
D.	Optical cover				Polycarbonate bubble, IK10 Rated

2.11	NETWORK SPECIFICATIONS
A.	RJ45					10/100BASE-TX, CAT-5
B.	SFP						100Base TX, SFP (fiber or copper)
C.	Management				OSA HTTP API, MX, SNMP v2, HTML (password 							protected)

2.12	ENVIRONMENTAL SPECIFICATIONS
A.	Operating temperature, Continuous		-49°F to +122°F (-45°C to +50°C)
B.	Operating Temperature, Max.		-49°F to +140°F (-45°C to +60°C)
C.	Humidity					10 to 90% RH, non-condensing
D.	MTBF					116,000 hrs, 30˚C; >61,000 hrs, at 50˚C, continuous use

2.13	CERTIFICATIONS AND RATINGS
A.	Waterproof standard			IP66
B.	Impact Resistance				IK10
C.	Regulatory
a.	IEC/ UL 60950-1
b.	IEC/EN 61000
c.	IEC/EN 55022 
d.	IEC/EN 55024
e.	FCC 
f.	RoHS

2.14		MANUFACTURER’S WARRANTY
A.	Repair or replacement of defective parts for a period of 2 years from date of shipment.

2.15	MODELS
A.	NTSC					Siqura HSD622 /N.
							IP high-speed PTZ dome camera, wide dynamic range, 							day/night, IP66, including sunshield.
B.	PAL 					Siqura HSD622 /P.  
							IP high-speed PTZ dome camera, wide dynamic range, 							day/night, IP66, including sunshield.
C.	Mounting Accessories
a.	Ceiling mounting - straight tube		Siqura CM01 (25 cm)
						Siqura CM02 (50 cm)
b.	Wall mounting-short			Siqura WM01A
c.	Wall Mt- Gooseneck tube		Siqura WM03A
d.	Box mounting				Siqura WM06
e.	Corner mounting			Siqura WM05
f.	Pole mounting- Thin			Siqura PM01
g.	Pole -Wide				Siqura PM02
h.	Pole thin box				Siqura PM03
i.	Pole wide box				Siqura PM04
j.	Swanneck (parapet)			Siqura PM05
k.	3rd Party Mt (1 ½” NPT adapter)		Siqura PTM01
l.	SFP modules				XSNet series or 3rd party 100Mb