A&E SPECIFICATION

PD1103Z2-EI
3 MEGAPIXEL INTELLIGENT IP OUTDOOR PTZ CAMERA WITH IR
TECHNICAL SPECIFICATIONS		SECURITY SYSTEM
DIVISION – 28 ELECTRONIC SAFETY AND SECURITY
LEVEL 1__28 20 00 ELECTRONIC SURVEILLANCE
LEVEL 2__28 23 00 VIDEO SURVEILLANCE
LEVEL 3__28 23 29 VIDEO SURVEILLANCE REMOTE DEVICES AND SENSORS

PART 2 - PRODUCTS
2.1	GENERAL
A.	This product shall be manufactured by a firm whose quality system is in compliance with the ISO-9001
B.	All equipment and materials used shall be standard components that are regularly manufactured and used in the manufacturer’s system.
C.	All systems and components shall have been thoroughly tested and proven in actual use.
D.	All systems and components shall be provided with comprehensive repair and spare parts replacement. The manufacturer on warranty and non-warranty items shall guarantee the spare parts and the repair.
E.	All systems and components must be in compliance with FCC, CE, UL and RoHS requirements.
2.2	3 MEGAPIXEL INTELLIGENT IP outdoor PTZ CAMERA WITH IR
A.	The network camera shall offer three video streams with up to 3MP resolution (2048 × 1536) in progressive scan CMOS format, with H.264 video compression.
B.	The network camera shall provide true & day night (ICR) low-light capabilities with sensitivity down to Color: 0.05 lux; B/W: 0.01 lux; 0 Lux with IR.
C.	The network camera shall support Back-Light Compensation (BLC) with selectable zones.
D.	The network camera shall offer video compression of H.264 and MJPEG. Three H.264 streams shall be supported with independent resolution, bit rate and frame rates for the main, sub and third streams.
E.	The network camera shall support enhanced H.264i compression to reduce bandwidth requirements.
F.	The camera shall offer weatherproof casing (rated IP66).
G.	The network camera shall include embedded Linux OS and support IE and client software for network preview, and be capable of performing firmware upgrades through a network using a software-based device utility or through the web interface.
H.	The network camera shall be equipped with built-in password protection which is not dependent on a server.
I.	The network camera shall not require a password during installation phase. Password protection will be activated after an administrator user account has been created.
J.	The network camera shall support standard IT protocols including: TCP/IP,ICMP,HTTP,HTTPS,FTP,DHCP,DNS,DDNS,RTP,RTSP,RTCP,PPPoE,NTP,UPnP, SMTP,SNMP,IGMP,802.1X,QoS,IPv6,Bonjour.
K.	The network camera shall support industry standard Hi Power over Ethernet (Hi-PoE) for powering the camera over the network in addition to 24 Vac local power.
L.	The camera shall provide the ability to take snapshot and record video clips from the web interface and store on the local computer.
M.	The camera shall support video motion detection with user defined areas and configurable sensitivity levels. In addition, the motion detection shall be supported by an arming schedule with the audible warning, surveillance center notification, email, ftp upload, and alarm output triggered as supported events.
N.	The camera’s web interface shall permit settings to be exported to and imported from a configuration file via the web interface and API.
O.	The camera shall be capable of performing firmware upgrades through a network using a software-based device utility or from the web interface.
P.	The camera shall conform to ONVIF, PSIA, CGI and ISAPI standards for integration with 3rd party video management systems (VMS). The camera may also support custom firmware for specific integration with a 3rd party VMS.
2.3	    PoWER
A.	Power Supply		24 Vac ± 10%, Hi-PoE (60 W)
B.	Power Consumption		Max. 60 W
2.4	Camera
A.	Image Sensor 		1/3” Progressive Scan CMOS
B.	Min. Illumination 		Color: 0.05 Lux @ (F1.6, AGC ON) 
				B/W: 0.01 Lux @ (F1.6, AGC ON)	
			  IR: 0Lux
C.	Shutter Speed 		1s to 1/30,000s
D.	Max. Image Resolution 		2048 × 1536
E.  Day & Night	  IR Cut Filter
F.  Day & Night Switch	Day, Night, Auto, Schedule, Triggered by alarm input are		selectable in Day/night Switch; two groups of parameters can	be set respectively for day and night
G. 	White Balance 	Auto, Manual, ATW, Indoor, Outdoor, Daylight Lamp, Sodium Lamp
H.	AGC 	  Auto, Manual
I.	S/N Ratio 	  ≥ 55 dB
J.	Back Light Compensation  	  On, Off
K.	HLC 	  On, Off
L.  WDR 	Wide dynamic range can be used when there is a high contrast of the bright area and the dark area of the scene: True WDR   120dB
M.  Defog                      On, Off
N.	Digital Zoom 	  16x
O.	Privacy Mask 	  24 privacy masks programmable
P. 	Digital Slow shutter	  Yes
Q.	Image settings	  Saturation, brightness, contrast, sharpness
R. 	Image rotation	  Mirror (center, off)
S.	Noise Reduction	  3D, selectable level (1-100)
T.	On screen Display	  Title (32 characters), Date, Time; User defined location
U.	OSD Display Modes	  Transparent, non-transparent; flashing, non-flashing

2.5	VIDEO & Audio SPECIFICATIONS
A.	Compression		      	Main stream: H.264
                            	Sub stream: H.264, MJPEG
							 	Third stream: H.264, MJPEG
B.  Three Streams 		Yes; Main stream up to 2048×1536; sub-stream up to 4CIF;	third stream up to 1280×720
C.	Resolutions supported       Main Stream: 
	50Hz: 50fps (2048 × 1536), 50fps@ (1920 × 1080), 25fps@ (1280 x 720)
	60Hz: 60fps (2048 × 1536), 60fps@ (1920 × 1080), 30 fps@   (1280 x 720)
	 Sub Stream:
	50Hz: 25fps@ (704×576, 352×288, 176×144)
	60Hz: 30fps@ (704×480, 352×240, 176×120)
Third Stream: 
			50Hz: 25fps@ (2048×1536, 1920×1080,1280×720, 704×576, 352×288, 176×144)
			60Hz: 30fps@ (2048×1536, 1920×1080,1280×720, 704×480, 352×240, 176×120)
D.  Video Bit Rate		32 Kbps ~ 16 Mbps
E.  Rate Control		      	Constant, Variable
F. 	ROI Encoding		Support 24 areas with adjustable levels
G. 	H.264 profiles		High, Main, Base
H.  Max. Frame Rate			50fps (2048 x 1536), 60fps (2048 x 1536)
I. 	H.264 profiles		      	Base Line Profile / Main Profile / High Profile
								H.264i intelligent compression
J.	Max. Frame Rate(main)   	30fps@2048×1536
K.  Audio Compression		G.711ulaw/G.711alaw/G.726/MP2L2/G.722
L.	Users
	1. Unicast		          	Up to 20 simultaneous users
	2. Multicast			      	Unlimited H.264
M.	Security Access		      	Password protected
N.	Software Interface	      	Web browser view and remote client.
2.6	Network
A.	Ethernet			10Base-T / 100Base-TX, RJ45 connector
B.	Protocols 	IPv4/IPv6, HTTP, HTTPS, 802.1X, QoS, FTP, SMTP, UPnP,   SNMP, DNS, DDNS, NTP, RTSP, RTP, TCP, UDP, IGMP, ICMP, DHCP, PPPoE
C.  Security                  	User authentication, Host authentication, IP address filtering 
D.  System Compatibility	   		ONVIF, PSIA, CGI, ISAPI
E.  RS485 protocol             Pelco-P, Pelco-D, self-adaptive
2.7	Connectors
A.  Communication interface     1 RJ45 10 M / 100 M Ethernet port
B.   RS-485 interface            Dry Contact
C.  Analog Output              1Vp-p Composite Output (75Ω/ BNC)
D.  Alarm Input                 Dry Contact
E.  Alarm Output                Dry Contact
F.  SD/SDHC slot               Up to 128GB; Manual REC / alarm REC
2.8	lens
A.	Focus Model 	  Auto, Semiautomatic, Manual
B.	Focal Length 	  4.5-162mm, 36x
C.	Zoom Speed	  Approx.3.3s (Optical Wide-Tele) 
D.	Angle of View	  60.6° ~ 3.68° (Wide-Tele)
E.	Min. Working Distance 	  10 ~ 1,500mm (Wide-Tele) 
F. 	Aperture Range 	  F1.6 – F4.4
2.9	pan and tilt
A.	Pan Range 				360° endless
B.	Pan Speed					Pan Manual Speed: 0.1° - 300°/s
							Pan Preset Speed: 540°/s
C.	Tilt Range				 	-20° ~ 90° (Auto Flip)
D.	Tilt Speed				 	Tilt Manual Speed: 0.1° ~ 240°/s
     						Tilt Preset Speed: 400°/s
E.	Proportional Zoom	Rotation speed can be adjusted automatically according to    zoom multiples
F.	Number of Preset		 	300
G.	Patrol 					16 patrols, up to 32 presets per patrol
H.	Pattern 	10 patterns, with the recording time not less than 10 minutes per pattern
I.	Power Loss Recovery		Support
J.	Park Action	Preset, Patrol, Pattern, Auto scan, Tilt scan, Random scan, Frame scan, Panorama scan
K.	PTZ Position Display 		On, Off
L.	Freeze Frame			 	Support
M.	Smart Tracking              Yes
N.	IR Illuminator				 Up to 200m effective range; variable by zoom level
2.10	INTELLIGENT FEATURES
A.	Motion Detection 	     		Normal mode and expert mode are available. In expert mode, 
				sensitivity and proportion of motion detection can be set for 8 
				regions and day or night
B.	Face Detection 	     		Human face that appears in the image can be recognized and 
					trigger e-mail, center or FTP linkage, and sensitivity of which 
					can be adjusted
C.  Audio Exception Detection  	As the sound of environment is abnormal, the device can 
recognize it and trigger alarm output
D.  Intrusion Detection  		4 regions of rectangular area can be set with different 
threshold, sensitivity and percentage
E.	Line Crossing Detection		4 lines can be set with different sensitivity to detect line 
				crossing behavior
F.	Region Entrance Detection		Enter a pre-defined virtual region from the outside place
G. 	Region Exiting Detection		Exit from a pre-defined virtual region
H.  Defocus Detection         	If focus of camera is changed, device can trigger alarm output
I.  Scene Change Detection		Arming schedule can be set for scene change detection; alarm 
				output can be linked
J.  ROI		Region of interest can be set as fixed area
K.	Defog		Defog can be turned on to get clear image in fog or haze
L.	VCA		VCA information can be written in streams, and back-end 
				devices can search for video clips contain specified type of 
				events
M.	Object Counting		Entrance and Exit object number is accounted and showed on 
					screen in real time (day/month/year based data chart can be 
					exported)
2.11	Alarm
A.	Alarm Input		7
B.	Alarm Output 		2 relay outputs, alarm response actions option
C.	Alarm Trigger	Face detection, Intrusion detection, Line crossing detection, Region entrance, Region exiting, Audio exception detection, Motion detection, Dynamic analysis, Tampering alarm, Network disconnect, IP address conflict, Storage exception
D.	Alarm Actions 	Preset, Patrol, Pattern, Micro SD/SDHC card recording, Relay output, Notification on Client
2.12	Input/Output
A.	Monitor Output 		1.0 V [p-p] / 75 Ω, NTSC (or PAL) composite, BNC
B.	Audio Input 		Mic in/Line in
  Line input: 2-2.4 V [p-p]; output impedance: 1 KΩ, ±10%
C.	Audio Output		Line level, impendence: 600 Ω
2.13	Web Browser Requirements
A.	Operating System		PC (Intel® Core® 2 Duo microprocessor, 2.6 GHz) with 
			Microsoft® Windows® XP, Windows Vista®, or Windows® 7 
B.	Web User Interface		   	DirectX for Windows XP, Windows Vista, Windows 7
C.	RAM 		                	2 GB
D.	Ethernet Card 		       	100 Mbps
E.	Web Brower		       	Internet Explorer® 7.0 or later; Firefox, Chrome
F. 	Screen Resolution 		   	1024 x 768 pixels or higher, 16- or 32-bit pixel color resolution
2.14	Client GUI
A.	Camera Control 	Pan/Tilt, Zoom, Focus, Click centering, Drag zoom, Iris, Preset   position call and program, Auto mode.
B.	OSD 		Up to 32 characters
C.	Date & Time Display 		Time: Week: Date, 3 formats on the Client
D.	Reading Patrol Message 	Display and reading of preset message contained in each patrol via client software
E.	Menu Language 		English
2.15	PHYSICAL
A. 	Operating Conditions		-40 °C ~ 65 °C (-40 °F ~ 149 °F) 
B.	Humidity		90% or less (non-condensing)
C. 	Dimension 		Ø 266 x 365 mm 
D.	Weight 		8 kg
E.  Mount Options	Long-arm wall mount; Corner mount; Pole mount
2.16	certifications and ratings
A.	Regulatory
a.	IEC/EN 61000
b.	IEC/EN 55022 
c.	IEC/EN 55024
d.	IEC /EN60950-1
e.	FCC Part 15, Class b
f.	UL/cUL 60950-1
g.	RoHS
B. 	Ratings
a.	Ingress Protection 	IP66
b.	Impact Protection  		 IK10
c.	Electrical Protection	TVS 6,000V lightning protection, surge protection and voltage transient protection
2.17	Models
PD1103Z2-EI